For RED Cameras please use their inbuilt Rec709 feature. You will find it in the RED RAW settings under ‘Gamma Curve’. Change this to Gamma 3.